# Welcome to fastAdc’s Documentation

Contents:

## Fast ADC Application

The Fast ADC application was developed to capture raw data of all ten ADCs channels and to process the information of pulse shaped signals. Each ADC signal is individually process according to the parameters configured by the user and the resulting data available via registers. In addition, 5 virtual channels are available which can be configure to be the sum or subtraction of two (real) ADC channels.

The application was developed under the Simulink environment, using the XFEL Simulink Library. As such, the application can be fully simulated in the Matlab environment using experimental data.

Tests of the system under experimental conditions have indicated that the device can reliably acquire 108000 raw samples, which corresponds to a time window of 1ms, from all 10 channels simultaneously.

In this documentation an overview of the hardware device (taken by the manual by EEE) is presented, as well as its setup in the configuration editor of the Karabo device. For more detail information on the board, firmware and performance results, please visit Fast Electronics Digitizer Overview page.

This chapter will cover the mininum requirements for the device to be operational, which is a Clock and Trigger signal.

FastADC Clock and Trigger Karabo parameters

### Clock Sources

The FastADC can accept clock signals from the following sources:

- TclkA (MicroTCA backplane)
- TclkB (MicroTCA backplane)
- Internal Clock (125 MHz)
- Front SMA Connector
- Front Hardlink Connector
- RJ45 SIS8900 RTM Connector

In XFEL, 99% of the FastADC setups use the TclkA or TclkB source, since these lines have a clock signal provided by the Timing Board, which is phase sync with the laser operation at XFEL.

### Trigger Sources

A trigger signal is required to start the operation of the Fast ADC Application. The Fast ADC firmware supports thirteen trigger sources, which can be combine to a single signal: eight from the MLVDS lines in the MicroTCA backplane, four from the Harlink connector, four from SIS8900 RTM RJ45 connector as well as an internal one.

Again, 99% of the XFEL FastADC setups use a trigger source from the MicroTCA Backplane, which is provided by the Timing system.

## Raw data

The fast ADC saves raw data from all 10 ADC channels simultaneously. The raw data is saved in the DDR memory available in the SIS8300 board. Some parameters can be tuned by the user to steer the data acquisition, and are presented in the figure below.

The amount of raw data saved with each trigger signal is configured in the Number of raw samples property in the Karabo device. It is possible to delay the raw data acquisition by a fixed number of samples after the trigger signal. This parameter is set by adjusting the Raw Delay property.

It is also possible to define the period of raw data acquisition (save one sample every N samples), which provides a zoom capability when observing raw data signals. As an example, if this register is set to 1, 2 or 3, the device will show an ADC value only every 2, 3 or 4 samples, respectively. The period of raw data acquisition is configured in the parameter Skip Samples. Notice that the parameters delay and period affect all ADCs signals raw data acquisition.

Example of an ADC signal and configuration parameters for raw data acquisition. The correspondent Karabo parameters are shown on the right.

The previous parameter affects the raw data acquisition for all channels. Nevertheless, to acquire raw data from a specific channel, the correspondent Enable Raw Data parameter must be set to TRUE in the channel options. Notice that a Signal Description can also be define by the user to easily identify the signal present in that channel.

Signal description and Enable Raw Data Karabo parameters for Channel 0.

### ADC Range

The ADC range can be configured to be 1.25, 1.5, 1.75 or 2.0 Voltage peak-to-peak. The setting can be changed when the device is not acquiring (STOP state), there is no need to re-initialize the device.

ADC range options.

### Time Axis

A time axis property is available for plotting Vector XY Graphs with the Raw data. The values take into account the Number of raw samples, Frequency and Skip Samples values configure in Karabo.

Time Axis property show in Karabo and the Vector XY Graph option in the Widget. After selecting this option, simply drag the Time axis parameter on top of the widget for the X axis to be updated with the time values.

### Virtual Channels

The FastADC includes 5 virtual channels (channel 10 through 14) which can be configured to be the sum or subtraction of two (real) ADC channels. The same features are available in these channels as any other ADC channels (peak integration, bunch pattern peak integration, multibaseline, adc alert, moving average, data voltage conversion, etc.).

Configuration of Channel 10 (Virtual). The channel is configure to be subtraction of the ADC signal in channel 0 and channel 9. The raw data graphs are display on the right.

## Integrator Processing Module

The fast ADC application includes, per ADC channel, an integrator processing module that can calculate the peak values of periodic ADC signals, or can be configured to integrate based on the current bunch pattern as described in the Bunch Pattern Decoding section. Each module can be individually configured. The following functionalities are available per ADC channel.

### Convert data to voltage units

Per channel, the Raw and Peak Integration data can be displayed in Voltage levels in Karabo, which taking into account the ADC Range configuration. Take note that the raw values are always saved in the DAQ.

Property to enable conversion of data to Voltage levels. Notice that all Raw properties are not converted.

### ADC Alert

An ADC alert can be configured per channel, which will be raised if the ADC signal goes above/below the user-specified threshold. To clear the alert, either disable it or reconfigure the threshold.

There is a Global ADC alert property which is true if any ADC channel alert is raised. To see which channel raised the alert, check the values in ADC Channels Alert.

ADC Alert Settings per channel (top) and Global ADC Alert (bottom).

### Signal Integration

To enable an Integrator module for a specific ADC channel, Enable Peak Computation must be set to True for that channel. Once enabled, the module waits for a trigger signal to start the calculation.

Peak signal calculation starts with the sample where the trigger signal is detected. It is possible to delay the calculation by a specific amount of data samples, by writing the desired value in the Pulse Delay property. For each peak, the module sums up as many ADC samples as specified in the Peak Samples property. The Number of pulses property configures the number of pulses to process after receiving a trigger, while the Pulse Period property specifies the number of samples expected between pulses (thus disentangling between pulses).

The calculated values are available in the output channel Channel X > Output > Schema > Data. Basic statistics are calculated in Karabo based on these values, including the mean and standard deviation of the peak values. The hardware also provides Max. ADC Sample vector, which contains the sample with highest (absolute) ADC value for each integrated peaks.

Another hardware calculated value, which is not saved in the output channel, is the Measured Peak range (located below the Pulse Period parameter). This value shows the difference (in counts or voltage) between the highest and lowest integrated peak.

Example of an ADC signal and of the configuration parameters for the integrator module.

### Baseline Configuration

The integrated values and statistics are calculated taking into account a baseline value. Multiple options for this value are available in the Baseline Settings node.

If a fixed baseline is desired, the value of the baseline should be input in the Fixed Baseline property, and the Enable fixed Baseline boolean should be set to true. Otherwise, the baseline will be calculated over a section of the signal.

A signal based Baseline can be calculate in the following ways:

Standard ::
  A single baseline value is calculated for the entire train. The Start of Baseline value delays the baseline calculation by a set value after the trigger signal.
Dynamic ::
  This setting is only available when using Bunch Pattern for Integration (see Bunch Pattern Decoding section). A single baseline value is calculated for the entire train. The Start of Baseline value delays the baseline calculation by a set value before the Sample First Bunch.
Multi value ::
  A baseline value is calculated for every pulse integrated. The Start of Baseline value delays the baseline calculation by a set value before the first sample used for integrated the pulse.

Baseline calculation and related Karabo Parameters

### Moving Average

The fast ADC firmware implements, per ADC channel, a 128 step moving average filter. The output of this filter, available in the Moving average settings node under the name Moving average, gives an indication of the order of magnitude of the ADC baseline value. To enable this filter, Enable Moving average must be set to ‘1’.

The firmware also provides values concerning the latest train of pulses received, which are referred to as train statistics. These values get updated whenever a new trigger signal is received. The calculated values are:

- Pulse delay (number of samples between trigger and first pulse),
- Minimum pulse width (in samples),
- Minimum pulse period (in samples),
- Number of pulses in last train.

and are presented in the figure here below:

Values calculated in each train.

To calculate these values, the moving average filter must be enabled and a threshold value configured in the ‘ADC Threshold magnitude’ property. Whenever the ADC signal goes above or below the threshold value (depending on whether the Moving average value), the firmware starts calculating the aforementioned values.

## Bunch Pattern Decoding

If desired, the FastADC can receive and decode the bunch pattern to know which bunches in a train are going to a specific beamline and/or have a pulse probe laser (PPL). Users can also specify a Max/Min of acceptable bunch charges. When enable and configure, the Bunch IDs and Charges are saved in the DAQ.

In addition, it is also possible to configure the FastADC to use this information to do Automatic Peak Integration or Conditional and/or Dynamic Raw acquisition.

### Settings

The decoding configuration is done in the device node Bunch Pattern Settings. The source of the X-ray bunch pattern to decode (Light Source parameter) can be any of SASE1, SASE2, SASE3, SASE1+3 or None. If bunch pattern decoding is enabled and None is selected, only the PPL bunch pattern will be considered. The Bunch pattern logic option defines whether a bunch ID is considered when there are bunches in both the X-ray beam and the PPL patterns (AND) or when there are bunches in either (OR).

Maximum and Minimum bunch charges can also be define.

If configure, during acquisition the Karabo device will update the First Bunch ID and Number of Bunches parameters in the current Train.

Bunch pattern settings in the FastADC and correspondent Output channel.

### Output

An output channel is also available, wherein a list containing the of bunch Ids determined by the conditions specified in the “Bunch Pattern Settings” node are output. This is DAQ compatible, but if DAQ recording is required it must be requested separately from the slow data of the device (request “<DeviceId>:bunchPatternNode.output” to be added to the data group.

### FastADC Calibration

To use the features described in the following sections, it is require to enable and configure the Bunch Pattern and calibrate the FastADC. This is done performing the following steps:

1. Stop acquisition of device
2. Set Raw Delay and all Peak Delay parameters to 0
3. Configure the Bunch Pattern according to your requirements
4. Configure the Pre Train Samples parameter if require (see Calibration for early bunches)
5. Start acquisition. Take note of the value in the property Sample First Bunch
6. Open the Karabo Trigger Middle Layer Device of the trigger used by the FastADC (check Board Configuration > Trigger Source property. When in doubt, contact Control and/or EEE colleagues)
7. Configure Macro P-Event property to be Standard Trigger
8. Change the Target Delay so that first peak sample (as desired for the peak integration) of the first bunch in the raw trace matches the Sample First Bunch value

Pre Train Samples and Sample First Bunch parameter.

#### Calibration for early bunches

For bunches which are present at the very beginning of the train, like PPL pulses, calibrating the FastADC following the previous section will result in a raw trace with very few samples before the train. This might not be desirable for setups which require data before the train arrives or use a signal based baseline(s).

To surpass this, the FastADC parameter Pre Train Samples can be used to configure an offset number of samples to acquire before the train.

### Automatic Peak Integration

Once the FastADC is calibrated (see previous section), channels can enable the Use the Bunch Pattern for peak computation feature. In this configuration, the FastADC automatically updates the Peak Integration parameters to integrate all the Bunches present in the Train that match the configuration of the Bunch Pattern.

The parameters Number of Pulses, Pulse Period and Pulse Delay are ignore by the device, since these will be updated by the hardware. The user only needs to specify:

- how many samples per peak the device should consider
- baseline configuration (see Baseline Configuration section)

Enable peak integration with the Bunch Pattern. Crossed are the parameters which are ignore in this setting

### Conditional and/or Dynamic Raw acquisition

With the FastADC calibrated (see FastADC Calibration), the property Raw Data Acquisition can be set to Conditional, meaning that raw data will only be taken if there are bunches in the train which match the configuration of the Bunch Pattern (please note that this applies to all channels). This parameter can also be set to Never, in case the user is only interested in values from peak integration.

When Raw Dynamic trigger is true, raw data acquisition will always start at sample number (Sample First Bunch - Raw Delay), meaning that acquisition will have a fix relation (time wise) with the first bunch in the train. This is similar to use the dynamic trigger from the timing system.

Using these features have no affect in the Automatic Peak Integration.

Conditional and Dynamic Raw Karabo properties

## Configure a fastAdc device

Please consider that the following configuration steps should be performed by experts; a wrong setting will result in a device not properly working.

### Configuration step by step

- Configuration
- Set Device File to the latest version of /dev/pciedevs?. Now we have pciedevs6 for SA2 and pciedevs7 for SCS;
- Set Map Directory to /home/xctrl/maps. This folder contains the configuration xml-files of the firmware registers.
- Change Board Configuration / FPGA Source Clock to TCLKA.
- Instantiate the fastAdc device. Now Train ID should be updating. If not or the value is some unreasonable number, please contact AE.
- By default, the channels are closed. To enable a channel, set Enable Peak Computation and Enable Raw Data to True.
- After you have done the previous steps correctly, Baseline Value and Mean Peak Value should be updating. If you have a scene, then you should see some noise. However, if nothing for the channel is updating and there is only a flat line in the scene (a single number), you are trapped by a bug in the firmware. Some discussions can be found in the redmine ticket #28462. You can fix it contacting AE. Anyway, the latest device release provides in the configuration editor the option to reset the DDR2 memory (in the SIS8300 board, where the raw ADC data are stored) and/or the ADC chip, clearing the above mentioned firmware bug.

## FastAdc

### Commands

Key | Displayed Name | Description | Alias | Access Level | Allowed States
--- | --- | --- | --- | --- | ---
dacNode.dacconfig | Update DAC parameters/memory | Update all DAC parameters in the hardware. |  | USER | ON
reset | Reset | Resets the device in case of an error |  | USER | ERROR
start | Start | Instructs device to go to started state |  | USER | ON
stop | Stop | Instructs device to go to stopped state |  | USER | ACQUIRING
trigger | Manual Trigger | Sends a software trigger to the hardware (always possible, independent of chosen trigger mode) |  | USER | ON
resetADC | Reset ADC | Reset ADC’s of FPGA in case of constant line, No signal |  | ADMIN | ERROR, ON
resetDDR2 | Reset DDR2 | Resets DDR2 in case of constant line, No signal |  | ADMIN | ERROR, ON

### Properties

Key | Displayed Name | Description | Alias | Type | Access Level | Access Mode | Allowed States
--- | --- | --- | --- | --- | --- | --- | ---
channel_0.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_0.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_0.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_0.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_0.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_0.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_0.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_0.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_0.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_0.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_0.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_0.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
channel_1.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_1.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_1.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_1.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_1.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_1.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_1.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_1.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_1.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_1.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_1.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_1.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
channel_2.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_2.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_2.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_2.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_2.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_2.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_2.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_2.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_2.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_2.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_2.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_2.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
channel_3.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_3.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_3.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_3.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_3.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_3.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_3.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_3.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_3.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_3.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_3.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_3.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
channel_4.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_4.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_4.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_4.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_4.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_4.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_4.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_4.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_4.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_4.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_4.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_4.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
channel_5.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_5.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_5.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_5.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_5.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_5.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_5.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_5.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_5.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_5.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_5.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_5.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
channel_6.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_6.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_6.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_6.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_6.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_6.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_6.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_6.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_6.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_6.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_6.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_6.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
channel_7.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_7.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_7.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_7.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_7.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_7.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_7.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_7.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_7.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_7.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_7.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_7.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
channel_8.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_8.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_8.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_8.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_8.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_8.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_8.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_8.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_8.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_8.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_8.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_8.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
channel_9.baseline | Baseline Value | Baseline Value. |  | Float | OBSERVER | READONLY |
channel_9.output.schema.data.baseline | Baseline Value | Baseline Value. |  | Double | OBSERVER | READONLY |
channel_9.output.schema.data.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Double | OBSERVER | READONLY |
channel_9.output.schema.data.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Double | OBSERVER | READONLY |
channel_9.output.schema.data.peaks | Peak Values | Vector of all peak values (with base line correction). |  | VectorFloat | OBSERVER | READONLY |
channel_9.output.schema.data.rawBaseline | Raw Baseline | Sums of baseline values from hardware |  | UInt32 | OBSERVER | READONLY |
channel_9.output.schema.data.rawData | Raw Data | Raw data from ADC. |  | VectorUInt16 | OBSERVER | READONLY |
channel_9.output.schema.data.rawPeaks | Raw Peaks | Sums of raw samples of selected peaks |  | VectorUInt32 | OBSERVER | READONLY |
channel_9.output.schema.data.samplesForBaseline | Samples For Baseline | Number of samples in rawBaseline |  | UInt32 | OBSERVER | READONLY |
channel_9.output.schema.data.samplesPerPeak | Samples Per Peak | Number of samples per peak |  | UInt32 | OBSERVER | READONLY |
channel_9.peakMean | Mean Peak Value | Mean of the Peak pulse (with base line correction). |  | Float | OBSERVER | READONLY |
channel_9.peakStd | Std. Dev. Peak Value | Standard deviation of the Peak pulse values (with base line correction). |  | Float | OBSERVER | READONLY |
dacNode.dacData | DAC Data | DAC data memory. |  | VectorInt32 | OBSERVER | READONLY |
dacNode.dacVoltageData | DAC Voltage Data | DAC data memory converted to Voltage |  | VectorDouble | OBSERVER | READONLY |
progress | Progress | The progress of the current action |  | Int32 | OBSERVER | READONLY |
trainId | Train ID | Current train ID as read from the FPGA |  | UInt64 | OBSERVER | READONLY |
triggerTime | Trigger Time | Time between Triggers |  | Int32 | OBSERVER | READONLY |
triggerTimeStat | Trigger Histogram | Histogram of time between Triggers |  | VectorUInt16 | OBSERVER | READONLY |
_connection_.brokers | Brokers | Brokers must be provided as URLs of format: tcp://<host>:<port>. Extra URLs serve as fallback. |  | VectorString | USER | INITONLY |
channel_0.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_0.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_0.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_0.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_0.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_0.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_0.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_0.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_0.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_0.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_0.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_0.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_0.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_0.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_1.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_1.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_1.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_1.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_1.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_1.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_1.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_1.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_1.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_1.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_1.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_1.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_1.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_1.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_2.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_2.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_2.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_2.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_2.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_2.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_2.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_2.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_2.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_2.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_2.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_2.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_2.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_2.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_3.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_3.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_3.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_3.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_3.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_3.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_3.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_3.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_3.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_3.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_3.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_3.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_3.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_3.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_4.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_4.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_4.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_4.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_4.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_4.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_4.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_4.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_4.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_4.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_4.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_4.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_4.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_4.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_5.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_5.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_5.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_5.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_5.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_5.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_5.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_5.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_5.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_5.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_5.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_5.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_5.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_5.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_6.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_6.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_6.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_6.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_6.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_6.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_6.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_6.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_6.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_6.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_6.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_6.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_6.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_6.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_7.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_7.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_7.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_7.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_7.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_7.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_7.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_7.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_7.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_7.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_7.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_7.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_7.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_7.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_8.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_8.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_8.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_8.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_8.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_8.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_8.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_8.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_8.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_8.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_8.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_8.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_8.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_8.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_9.baseStart | Start of Baseline | Starting Sample to calculate the Baseline. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_9.baseStop | End of Baseline | Ending Sample of the Baseline calculation. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_9.calibrationFactor | Calibration Factor | Factor to be used with all peak values and the related mean and std values |  | Double | USER | RECONFIGURABLE | ON
channel_9.enablePeakComputation | Enable Peak Computation | Enable peak computation on the FPGA. |  | Bool | USER | RECONFIGURABLE | ON
channel_9.enableRawDataStreaming | Enable Raw Data | Enable streaming out of raw data. |  | Bool | USER | RECONFIGURABLE | ON
channel_9.fixedBaseline | Fixed Baseline | If fixed baseline is enabled, this value will be used for calculations instead of the base line from the h/w. |  | Double | USER | RECONFIGURABLE | ON
channel_9.fixedBaselineEna | Enable fixed Baseline | Enables the use of a fixed baseline value. |  | Bool | USER | RECONFIGURABLE | ON
channel_9.initialDelay | Pulse Delay | Time delay between trigger and start of processing algorithm. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_9.numPulses | Number of pulses | Number of pulses expected in each trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_9.output.distributionMode | Distribution Mode | Describes the policy of how to fan-out data to multiple (shared) input channels |  | String | USER | INITONLY |
channel_9.output.hostname | Hostname | The hostname to which connecting clients will be routed to |  | String | USER | INITONLY |
channel_9.output.noInputShared | No Input (Shared) | What to do if currently no share-input channel is available for writing to |  | String | USER | INITONLY |
channel_9.peakSamples | Peak Samples | Number of peak samples in each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
channel_9.pulsePeriod | Pulse Period | Number of samples between each pulse. |  | UInt32 | USER | RECONFIGURABLE | ON
config.fpgaClock | FPGA Source Clock | Source Clock to FPGA operations. |  | String | USER | INITONLY |
config.softTrigTime | Soft Trigger Interval | Interval between software generated triggers in milli seconds. |  | UInt32 | USER | RECONFIGURABLE | ON
config.triggerSource | Trigger Source | Source of trigger for algorithm (RX17 to TX20 - Backplane; Front1-4 - Harlink Front Panel). |  | String | USER | INITONLY |
dacNode.dacCyclesSamples | DAC Cycles per Samples | Number of clock cycles per Samples. |  | UInt32 | USER | RECONFIGURABLE | ON
dacNode.dacDataMode | Select DAC Data Mode | False: binary offset; True: 2 complement |  | Bool | USER | RECONFIGURABLE | ON
dacNode.dacFile | DAC File | File with DAC values. |  | String | USER | RECONFIGURABLE | ON
dacNode.dacSkipSamples | DAC Skip Samples | Number of DAC samples to be in output. |  | UInt32 | USER | RECONFIGURABLE | ON
dacNode.dacTrigger | DAC Internal Trigger | Enable DAC Internal Trigger. |  | Bool | USER | RECONFIGURABLE | ON
dacNode.dacTriggerPeriod | DAC Internal Trigger Period | Period of internal DAC Trigger. |  | UInt32 | USER | RECONFIGURABLE | ON
dacNode.enableDAC | Enable DAC | Enable DAC channel. |  | Bool | USER | RECONFIGURABLE | ON
dacNode.voltageIntercept | Voltage Conversion (y-intercept) | Value of intercept for converting DAC to Voltage value |  | Double | USER | RECONFIGURABLE | ON
dacNode.voltageSlope | Voltage Conversion (slope) | Value of slope for converting DAC to Voltage value |  | Double | USER | RECONFIGURABLE | ON
delay | Raw Delay | Time delay between trigger and start of raw data acquisition. |  | UInt32 | USER | RECONFIGURABLE | ON
deviceFile | Device File | Device driver file to access the hardware (e.g. /dev/pciedevs9). |  | String | USER | RECONFIGURABLE | ERROR
mapDirectory | Map Directory | Folder where all xml mapping files are located. |  | String | USER | RECONFIGURABLE | ERROR
numberRawSamples | Number of raw samples | Number of raw samples to aquire, per channel, with each start of raw data acquisition. |  | UInt32 | USER | RECONFIGURABLE | ON
skipSamples | Skip Samples | If 1/2/3/…, show only every 2nd/3rd/4th/… raw ADC value (i.e. “zoom out”). |  | UInt32 | USER | RECONFIGURABLE | ON
channel_0.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_0.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
channel_1.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_1.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
channel_2.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_2.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
channel_3.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_3.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
channel_4.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_4.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
channel_5.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_5.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
channel_6.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_6.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
channel_7.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_7.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
channel_8.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_8.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
channel_9.output.compression | Compression | Configures when the data is compressed (-1 = off, 0 = always, >0 = threshold in MB |  | Int32 | EXPERT | INITONLY |
channel_9.output.port | Port | Port number for TCP connection |  | UInt32 | EXPERT | INITONLY |
interfaces | interfaces |  |  | VectorString | EXPERT | READONLY |
performanceStatistics.enable | Enable Performance Indicators | Enables some statistics to follow the performance of an individual device |  | Bool | EXPERT | RECONFIGURABLE |
performanceStatistics.maxEventLoopLatency | Max. event loop latency | Maximum time interval between posting a message on the central event loop and processing it within averaging interval. |  | UInt32 | EXPERT | READONLY |
performanceStatistics.maxProcessingLatency | Maximum latency | Maximum processing latency within averaging interval. |  | UInt32 | EXPERT | READONLY |
performanceStatistics.messagingProblems | Messaging problems | If true, there is a problem consuming broker messages |  | Bool | EXPERT | READONLY |
performanceStatistics.numMessages | Number of messages | Number of messages received within averaging interval. |  | UInt32 | EXPERT | READONLY |
performanceStatistics.processingLatency | Processing latency | Average time interval between remote message sending and processing it in this device. |  | Float | EXPERT | READONLY |
useTimeserver | Use Timeserver | Unused - whether device connects to time server is configured via ‘timeServerId’ |  | Bool | ADMIN | INITONLY |

# Indices and tables

Read the Docs v: master

Versions
  master
  latest
  fix-requirements

Downloads
  pdf
  html
  epub

On Read the Docs
  Project Home
  Builds

Free document hosting provided by Read the Docs.